Skid Steer Loader Daily Inspection Checklist

|  |
| --- |
| **Skid Steer Loader Daily Inspection Checklist** |
| Company Name: | Date: |
| Operator Name: | Site: |
| Machine Number: |
| **Check Type** (please circle) | Pre-Start | Post-Operational |

|  |  |  |  |
| --- | --- | --- | --- |
| **Component** | **What to Check for** | **✓** | **Comments** |
| **External Check** |
| Tyres and wheels (if applicable). | Inflation, pressure, damage, covers. |  |  |
| Tracks and drive lugs (if applicable). | Damage, tension, cuts, foreign materials. |  |  |
| Lift arms, pins, and coupler. | Wear, damage, leaks, loose parts. |  |  |
| Bucket and linkage | Wear, damage, cracks, leaks, loose parts, excessive debris. |  |  |
| Underneath machine. | Leaks, loose parts, damage. |  |  |
| Frame, steps, handholds. | Condition, damage, cleanliness. |  |  |
| Hydraulic cylinders, tubes, hoses, fittings. | Damage and leaks. |  |  |
| Covers and guards | Damage, wear, secured. |  |  |
| Windows and mirrors. | Cleanliness, damage, visibility. |  |  |
| Decals and signage. | Readability, wear. |  |  |
| Load capacity plate. | Damage, wear, visible. |  |  |
| Overall machine. | Loose or missing parts, damage, wear, missing guards and safety devices. |  | **Out of Service Tag Attached? Yes / No** |
| **Engine Check** |
| Fluids. | Engine oil, hydraulic oil, transmission oil, coolant, engine pre-cleaner, brake fluid. |  |  |
| Batteries. | Cleanliness, loose nuts/bolts. |  |  |
| Air filter. | Damage, dirt build up, indicators. |  |  |
| Radiator.  | Damage, leaks, dirt build up, blockages. |  |  |
| Hoses. | Leaks, wear, damage. |  |  |
| Belts. | Tightness, wear, cracks. |  |  |
| Overall engine. | Damage, dirt build up, leaks. |  | **Out of Service Tag Attached? Yes / No** |
| **Internal/Cabin Check** |
| Levers, controls and gauges. | Damage, cleanliness, labels, working. |  |  |
| ROPS. | Damage, cracks, wear. |  |  |
| Floor plates.  | Clear and free of oil/grease. |  |  |
| Seat and seat belts. | Adjustment, damage, wear. |  |  |
| Fire extinguisher. | Damage and charge. |  |  |
| Logbook, running sheet, vehicle history, service sheets.  | Present and correct |  |  |
| Mirrors. | Adjusted, clean, visible. |  |  |
| Overall cabin interior. | Cleanliness, damage, missing parts. |  | **Out of Service Tag Attached? Yes / No** |
| **Operational Checks** |
| Master and isolation switches, start switch or key | Present, functioning, damage. |  |  |
| Joy sticks or levers | Functioning, damage, wear. |  |  |
| Accelerator and brakes, emergency stopping device | Working, damage, wear, dirt build up on pedals. |  |  |
| Bucket. | Movements, smooth or jerky. |  |  |
| Air-conditioning, radio, two-way radios, lights, horn. | Functioning, damage, wear. |  |  |
| Gauges. | Oil pressure, fuel level, engine temperature, hydraulics, and speedometer. |  |  |
| Start-up alarms. | Functioning and visible. |  |  |
| GPS, auto levelling controls. | Working, visible, accurate, damage, wear. |  | **Out of Service Tag Attached? Yes / No** |

|  |
| --- |
| **Action Taken to Repair Skid Steer Loader:** |
| Name: | Date of Repair: |

|  |
| --- |
| **Action Taken to Repair Skid Steer Loader:** |
| Comments: |
| Supervisor Name: | Signature: | Date: |